Supplementary Information for: Glacial sedimentation, fluxes and erosion rates associated with ice retreat in Petermann Fjord and Nares Strait, NW Greenland

Kelly A. Hogan1,2, Martin Jakobsson3,4 , Larry Mayer2, Brendan Reilly5, Anne Jennings6, Alan Mix5, Tove Nielsen7, Katrine J. Andresen8, Egon Nørmark8, Katrien Heirman7,10, Elina Kamla7,9, Kevin Jerram2, Christian Stranne3,4

1British Antarctic Survey, Natural Environment Research Council, High Cross, Madingley Road, Cambridge, CB3 0ET, UK

2 Center for Coast and Ocean Mapping, University of New Hampshire, NH 03824, USA

3 Department of Geological Sciences, Stockholm University, 10691 Stockholm, Sweden

4 Bolin Centre for Climate Research, Stockholm University, Stockholm 106 91, Sweden

5 College of Earth, Ocean, and Atmospheric Sciences, Oregon State University, Corvallis, OR 97331, USA

6 Institute of Arctic and Alpine Research, University of Colorado, Boulder, CO 80309-0450, USA

7 Geological Survey of Denmark and Greenland, Øster Voldgade 10, 1350 Copenhagen K, Denmark

8 Department of Geoscience, Aarhus University, Hoegh-Guldbergs Gade 2, DK-8000, Aarhus C, Denmark

9 TNO, Geological Survey of the Netherlands, Princetonlaan 6, NL-3584 CB Utrecht, The Netherlands

10 Rambøll Management Consulting, Hannemanns Allé 53, DK-2300 Copenhagen S, Denmark

*Correspondence to*: Kelly A. Hogan (kelgan@bas.ac.uk)


# Drainage basins for glacial erosion rate calculations

In order to estimate glacial erosion rates for the Petermann Ice Stream and other Greenland outlet glaciers for comparison the area of the glacier catchment or drainage basin area (*Adr*) is required (see Equation 1 in the main text). For subglacial erosion to occur the ice sheet must be moving over the bed, i.e. ice cannot be frozen to the bed and, therefore, we exclude areas where ice velocities are <50 m a-1. For Petermann and Jakobshavn glaciers, the erosion rates that we calculate are for a period during deglaciation. Thus, in the absence of ice-sheet velocities for a deglacial ice sheet (modelled or otherwise inferred), we utilise ice-sheet velocities from the modern Greenland Ice Sheet (GrIS) to define the drainage basin areas for these catchments. Modern GrIS velocities for the Petermann, Jakobshavn and Kangerlussuaq glacier systems are from the MEaSUREs Greenland Ice Velocity: *Selected Glacier Site Velocity Maps from Optical Images, Version 2* dataset for 2017-2018 (Howat, 2017). In both catchments we extend the drainage basin to include the part of the fjord up to the fjord-mouth sill but now not occupied by ice (Supplementary Fig. 1a, b). The northern and southern boundaries of the Jakobshavn drainage basin were digitised from the Zwally et al. (2012) drainage system divides. For calculations for Kangerdlugssuaq Glacier, East Greenland, we have also modified the drainage basin area to only include areas not frozen to the bed as discussed in the main text (Supp. Fig. 1c).

# References

Howat, I. M.: MEaSUREs Greenland Ice Velocity: Selected Glacier Site Velocity Maps from Optical Images, Version 2, Howat, I. M. (Ed.), NASA National Snow and Ice Data Center Distributed Active Archive Center. Ice Velocity, Boulder, Colorado USA. , 2017.

Zwally, J. H., Giovinetto, M.B., Beckley, M.A., and Saba, J.L.: Antarctic and Greenland Drainage Systems, GSFC Cryospheric Sciences Laboratory, at <http://icesat4.gsfc.nasa.gov/cryo_data/ant_grn_drainage_systems.php>, 2012.



Supplementary Figure 1. Maps of Greenland outlet glaciers discussed in main text showing modern ice-sheet velocities (Howat, 2017) with drainage basins (black lines) and areas used in glacial erosion rate calculations for: (a) Petermann Glacier, Northwest Greenland; (b) Jakobshavn Isbrae, West Greenland; (c) Kangerdlugssuaq Glacier, East Greenland.